### A good answer might be:

The program assumes that all calculations fit into 32 bits.

# End of Chapter

You have reached the end of this chapter. Click on a blue subject to go to where it was discussed. To get back here, click on the "back arrow" button of your browser.

- Mnemonic register names.
- The assembler temporary register.
- The kernel of an operating system.
- Systems software and symbolic addresses.
- Pseudoinstructions and the pseudocomputer.
- The move pseudoinstruction.
- The la pseudoinstruction.
- lw pseudoinstruction.
- sw pseudoinstruction.
- nop pseudoinstruction.

You have reached the end of the chapter.