### A good answer might be:

    FEED      1111 1110 1110 1101
    BECA      1011 1110 1100 1010
    ----      ---- ---- ---- ----
    4027      0100 0000 0010 0111

# NOR Instruction

NOR Operation on Bits
first operand | 0 | 0 | 1 | 1
second operand | 0 | 1 | 0 | 1
| __ | __ | __ | __
result | 1 | 0 | 0 | 0

There is a bitwise NOR instruction. There is no immediate operand NOR instruction. NOR is equivalent to performing the OR operation, then complementing the bits (change 0 to 1 and 1 to 0). Here is the assembly language for it:

    nor  d,s,t    # $d <-- bitwise NOR
                  # between $s with $t.

### QUESTION 10:

What is the bitwise NOR of the following?

    FEED
    BECA
    ----