### A good answer might be:

Use "less than" with the operations reversed.

# Branch Instructions

The floating point branch instructions inspect the condition bit in the coprocessor. The `bc1t` instruction takes the branch if the bit is true (==1). The `bc1t` instruction takes the branch if the bit is false (==0). These are the only two floating point branch instructions.

Instruction | Operation
--- | ---
`bc1t label` | branch to `label` if the coprocessor 1 condition bit is true
`bc1f label` | branch to `label` if the coprocessor 1 condition bit is false

The branch instructions have a one instruction branch delay. Hardware requires a `nop` instruction after each branch instruction. For this chapter, let us not bother with this. When running the programs with SPIM, disable branch delays in the settings menu.

### QUESTION 4:

Where does execution of the `bc1t` instruction take place? In the FPU or the CPU?