Which byte of $9 should go into address $0x10000000?

### A good answer might be:

0x12 --- the "big end" of an integer goes into the first address of a group of bytes with big-endian byte order.

Eventually, after a few more right shifts, it gets there.

# Loading Halfwords

A MIPS halfword is two bytes. This, also, is a frequently used length of data. In ANSI C, a short integer is usually two bytes. So, MIPS has instructions to load halfword and store halfwords.

There are two load halfword instructions. One extends the sign bit of the halfword in memory into the upper two bytes of the register. The other extends with zeros.

    lh   t,off(b)   # $t <-- Sign-extended halfword
                    # starting at memory address b+off.
                    # b is a base register.
                    # off is 16-bit two's complement.

    lhu  t,off(b)   # $t <-- zero-extended halfword
                    # starting at memory address b+off.
                    # b is a base register.
                    # off is 16-bit two's complement.

Halfword addresses must be halfword aligned. Attempting to load a halfword from an unaligned address will cause a trap.

### QUESTION 7:

How can you tell if an address is halfword aligned?