### A good answer might be:

What is the symbolic address of the first byte of the `.data` section? tape What main storage address will it have at run time? 0x10000000

The main storage address for the first byte of the data section is 0x10000000 by default (of the SPIM assembler). There is nothing in the program that says this.

# A Run of the Program

The SPIM display shows data in groups of 4-byte words with the most significant byte on the left. This makes the data readable by humans. Within each group of four, the byte with the lowest address is on the right. Here is how SPIM looks after the first byte of the register has been stored to the buffer:

The byte is where it should be in memory, although you have to look at the display carefully to see this.

### QUESTION 6:

Which byte of $9 should go into address $0x10000000?