Does the `sra` instruction work correctly for unsigned integers?

### A good answer might be:

No. For unsigned integers the "sign bit" should not be replicated.

# End of Chapter

You have reached the end of this chapter. Click on a blue subject that has your undivided attention to go to where it was discussed. To get back here, click on the "back arrow" button of your browser.

- The number of places resulting from an integer multiplication.
- The number of places resulting from an integer division.
- The hi and lo registers.
- The mult and multu instructions.
- The mfhi and mflo instructions.
- The div and divu instructions.
- Arithmetic shift right.
- The sra instruction.

Go to Table of Contents

You have reached the end of the chapter.