### A good answer might be:

`ori $8,$9,0x004A`
31....26 | 25...21 | 20...16 | 15...................0
0xD | s | d | unsigned const
0xD | 0x9 | 0x8 | 0x004A

# Individual Field Values

There are four fields in the instruction. We know the bit pattern that goes into each field. Let us put those patterns in registers $11, $12, $13, and $14. The program starts out:

    or    $25,$0,$0        # clear $25
    ori   $11,$0,________  # opcode
    ori   $12,$0,________  # operand $s
    ori   $13,$0,________  # dest. $d
    ori   $14,$0,________  # immediate operand

### QUESTION 16:

Fill in the fields.