What assembly language instruction clears register $25 ?

### A good answer might be:

    or  $25,$0,$0        # $25 <-- $0

(There are others that also work for this).

# Target Instruction

The program starts with:

    or  $25,$0,$0        # clear $25

Now the correct bit patterns are placed into the fields of the instruction. The instruction we are assembling is:

    ori  $8,$9,0x004A

### QUESTION 15:

Fill in the fourth row with the bit patterns. Use hexadecimal (assume that the bit patterns are truncated on the left to make them the right size).

`ori $8,$9,0x004A`
31....26 | 25...21 | 20...16 | 15...................0
0xD | s | d | unsigned const